1- No need to switch the module to serial port mode (keep it in I2C mode).
2- Connect the converter to PC and open the upgrade tool.
3-Choose the serial port number and click 'CONNECT'. Then open the bin file
4- Connect the Lidar to the converter. Note: connect only the GND, RX and TX and leave the VCC unconnected at this stage
5- Click 'DOWNLOAD' on the panel of the upgrade tool and conncet the VCC of the Lidar to the converter within 10s.
[image: image1.jpg]‘ 110200 Connect

Bin Fil

Idle





When it is done, you may check the version number of the firmware.

Don't forget to power off the LiDAR after the total upgrading method
